CK WORLDWIDE TIG TORCH POWER GAS COOLED CONNECTORS

FITS POWER CABLES WITH A MALE THREAD 3/8”-24 RIGHT HAND

If your machine has the gas flow through the female power connection then you would use the GAS-THRU Connector.

A diagram of a welding torch

AI-generated content may be incorrect.

|  |
| --- |
|  |